(librepcb_component 2de097de-aef3-457e-924b-1bb16f8835f5
 (name "WS2812D-F5")
 (description "Programmable LED; 5mm; RGB; 1.82.2/2.83.1/2.93.2V; -2580C\nSource: Datasheet")
 (keywords "eagle,import")
 (author "EAGLE Import")
 (version "0.1")
 (created 2026-03-15T22:07:44Z)
 (deprecated false)
 (generated_by "EagleImport::::WS2812D-F5")
 (category 70421345-ae1d-4fed-aa60-e7619524b97f)
 (schematic_only false)
 (default_value "{{ MPN or DEVICE or COMPONENT }}")
 (prefix "LED")
 (signal fe65bec8-494a-480b-83f5-ac911f0cd25d (name "ANODE_(R/G/B_LED)") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal d24a7578-0b48-4f7f-ac45-6d490570a117 (name "CATHODE") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal abca830a-0137-4e61-a368-8538df532a68 (name "DIN") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal f1783386-b797-463c-b275-91475aa958dd (name "DOUT") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (variant e8f17341-643a-470a-8663-9f46cdd2e235 (norm "")
  (name "default")
  (description "")
  (gate d862b9b0-cdbc-4597-9d55-e7753e9b291f
   (symbol 6f3ffd75-874d-4faf-a742-fde278959dd6)
   (position 0.0 0.0) (rotation 0.0) (required true) (suffix "")
   (pin 0b70c729-2fe4-40c8-b40c-9630d1ff2629 (signal abca830a-0137-4e61-a368-8538df532a68) (text signal))
   (pin a42d783b-b8b9-4cb9-9c88-027504a3fa33 (signal fe65bec8-494a-480b-83f5-ac911f0cd25d) (text signal))
   (pin be6a8872-838e-42ea-be90-3dd2266f9bd1 (signal f1783386-b797-463c-b275-91475aa958dd) (text signal))
   (pin f3c16b44-db63-4852-8529-549a52852cff (signal d24a7578-0b48-4f7f-ac45-6d490570a117) (text signal))
  )
 )
)
