(librepcb_component 2b24b18d-bd95-4fb4-8fe6-bce1d020ead4
 (name "LED")
 (description "Single LED")
 (keywords "")
 (author "U. Bruhin")
 (version "0.2")
 (created 2015-03-08T16:21:14Z)
 (deprecated false)
 (generated_by "")
 (category 70421345-ae1d-4fed-aa60-e7619524b97f)
 (schematic_only false)
 (default_value "{{MPN or COLOR}}")
 (prefix "LED")
 (attribute "COLOR" (type string) (unit none) (value ""))
 (signal f1467b5c-cc7d-44b4-8076-d729f35b3a6a (name "A") (role passive)
  (required true) (negated false) (clock false) (forced_net "")
 )
 (signal 7b023430-b68f-403a-80b8-c7deb12e7a0c (name "C") (role passive)
  (required true) (negated false) (clock false) (forced_net "")
 )
 (variant ed0f0ca2-43ff-4a10-94c2-2958bc336586 (norm "")
  (name "default")
  (description "")
  (gate 80e56299-8f8c-4613-a559-1fba31f01411
   (symbol cb442e56-0ec7-4486-8c43-7bdfa9b47d9a)
   (position 0.0 0.0) (rotation 0.0) (required true) (suffix "")
   (pin 18de942d-8b47-4daf-9e07-d089204e09d0 (signal 7b023430-b68f-403a-80b8-c7deb12e7a0c) (text none))
   (pin 2a64f851-340a-43f2-b1cf-06a1d4b54560 (signal f1467b5c-cc7d-44b4-8076-d729f35b3a6a) (text none))
  )
 )
)
