(librepcb_device 698883e7-e78f-4385-807c-8307c338c6c2
 (name "LED ⌀5.0x8.7/2.54mm Green")
 (description "Generic through-hole LED with 5.00 mm body diameter.\n\nBody height: 8.70 mm\nLead spacing: 2.54 mm\nStandoff: 1.00 mm\nBody color: Green\n\nGenerated with librepcb-parts-generator (generate_led.py)")
 (keywords "led,tht")
 (author "U. Bruhin")
 (version "0.1.1")
 (created 2022-08-31T11:18:33Z)
 (deprecated false)
 (generated_by "")
 (category 70421345-ae1d-4fed-aa60-e7619524b97f)
 (component 2b24b18d-bd95-4fb4-8fe6-bce1d020ead4)
 (package 3e3d69b7-47dc-41fc-b077-bc61a0651b6c)
 (pad 1aba7a03-0f52-4355-9890-635346e5c72c (optional false)
  (signal 7b023430-b68f-403a-80b8-c7deb12e7a0c)
 )
 (pad c4a1e84b-9ac4-4dca-85c1-91a6340b3e26 (optional false)
  (signal f1467b5c-cc7d-44b4-8076-d729f35b3a6a)
 )
)
