(librepcb_package 951816e7-28c0-478e-b4fa-87490c1519c3
 (name "Pin Socket 2.54mm 2x04 ⌀1.0mm")
 (description "A generic 2x4 female pin socket with 2.54mm pin spacing and 1.0mm drill holes.\n\nGenerated with librepcb-parts-generator (generate_connectors.py)")
 (keywords "connector, 2x4, d1.0, pin socket, female header, tht")
 (author "Danilo B.")
 (version "0.3")
 (created 2019-09-17T20:00:41Z)
 (deprecated false)
 (generated_by "")
 (category 6183d171-e810-475a-a568-2a270aff8f5e)
 (assembly_type tht)
 (grid_interval 2.54)
 (min_copper_clearance 0.2)
 (pad 2c523853-9440-44c7-81ae-c11c7fe25cd6 (name "1"))
 (pad 4bf0bf2a-5618-4be3-90d0-fb0c5466d408 (name "2"))
 (pad dcdcadb6-3a0f-4d2d-8f2e-7983bab71f66 (name "3"))
 (pad fdeb5f05-0729-4338-983a-91a85b87bc5c (name "4"))
 (pad 79e276a3-4809-47ce-a8dd-7c7dd934f718 (name "5"))
 (pad 0915229d-ce34-4a3b-af68-a81bcfdf23b6 (name "6"))
 (pad f8d07c9c-d06f-4b3e-8521-86e33fe9d5a3 (name "7"))
 (pad 0e2a8d54-61a3-4204-9bf1-edf049c03ef1 (name "8"))
 (3d_model febc544f-ffca-40fa-a91a-9e40818a6348 (name "Pin Socket 2.54mm 2x04 ⌀1.0mm"))
 (footprint fbfe3b7f-2737-43f7-9998-64e8c405850e
  (name "default")
  (description "")
  (3d_position 0.0 0.0 0.0) (3d_rotation 0.0 0.0 0.0)
  (3d_model febc544f-ffca-40fa-a91a-9e40818a6348)
  (pad 2c523853-9440-44c7-81ae-c11c7fe25cd6 (side top) (shape roundrect)
   (position -1.27 3.81) (rotation 0.0) (size 2.19 1.587) (radius 0.0)
   (stop_mask auto) (solder_paste off) (clearance 0.0) (function standard)
   (package_pad 2c523853-9440-44c7-81ae-c11c7fe25cd6)
   (hole 2c523853-9440-44c7-81ae-c11c7fe25cd6 (diameter 1.0)
    (vertex (position 0.0 0.0) (angle 0.0))
   )
  )
  (pad 4bf0bf2a-5618-4be3-90d0-fb0c5466d408 (side top) (shape roundrect)
   (position 1.27 3.81) (rotation 0.0) (size 2.19 1.587) (radius 1.0)
   (stop_mask auto) (solder_paste off) (clearance 0.0) (function standard)
   (package_pad 4bf0bf2a-5618-4be3-90d0-fb0c5466d408)
   (hole 4bf0bf2a-5618-4be3-90d0-fb0c5466d408 (diameter 1.0)
    (vertex (position 0.0 0.0) (angle 0.0))
   )
  )
  (pad dcdcadb6-3a0f-4d2d-8f2e-7983bab71f66 (side top) (shape roundrect)
   (position -1.27 1.27) (rotation 0.0) (size 2.19 1.587) (radius 1.0)
   (stop_mask auto) (solder_paste off) (clearance 0.0) (function standard)
   (package_pad dcdcadb6-3a0f-4d2d-8f2e-7983bab71f66)
   (hole dcdcadb6-3a0f-4d2d-8f2e-7983bab71f66 (diameter 1.0)
    (vertex (position 0.0 0.0) (angle 0.0))
   )
  )
  (pad fdeb5f05-0729-4338-983a-91a85b87bc5c (side top) (shape roundrect)
   (position 1.27 1.27) (rotation 0.0) (size 2.19 1.587) (radius 1.0)
   (stop_mask auto) (solder_paste off) (clearance 0.0) (function standard)
   (package_pad fdeb5f05-0729-4338-983a-91a85b87bc5c)
   (hole fdeb5f05-0729-4338-983a-91a85b87bc5c (diameter 1.0)
    (vertex (position 0.0 0.0) (angle 0.0))
   )
  )
  (pad 79e276a3-4809-47ce-a8dd-7c7dd934f718 (side top) (shape roundrect)
   (position -1.27 -1.27) (rotation 0.0) (size 2.19 1.587) (radius 1.0)
   (stop_mask auto) (solder_paste off) (clearance 0.0) (function standard)
   (package_pad 79e276a3-4809-47ce-a8dd-7c7dd934f718)
   (hole 79e276a3-4809-47ce-a8dd-7c7dd934f718 (diameter 1.0)
    (vertex (position 0.0 0.0) (angle 0.0))
   )
  )
  (pad 0915229d-ce34-4a3b-af68-a81bcfdf23b6 (side top) (shape roundrect)
   (position 1.27 -1.27) (rotation 0.0) (size 2.19 1.587) (radius 1.0)
   (stop_mask auto) (solder_paste off) (clearance 0.0) (function standard)
   (package_pad 0915229d-ce34-4a3b-af68-a81bcfdf23b6)
   (hole 0915229d-ce34-4a3b-af68-a81bcfdf23b6 (diameter 1.0)
    (vertex (position 0.0 0.0) (angle 0.0))
   )
  )
  (pad f8d07c9c-d06f-4b3e-8521-86e33fe9d5a3 (side top) (shape roundrect)
   (position -1.27 -3.81) (rotation 0.0) (size 2.19 1.587) (radius 1.0)
   (stop_mask auto) (solder_paste off) (clearance 0.0) (function standard)
   (package_pad f8d07c9c-d06f-4b3e-8521-86e33fe9d5a3)
   (hole f8d07c9c-d06f-4b3e-8521-86e33fe9d5a3 (diameter 1.0)
    (vertex (position 0.0 0.0) (angle 0.0))
   )
  )
  (pad 0e2a8d54-61a3-4204-9bf1-edf049c03ef1 (side top) (shape roundrect)
   (position 1.27 -3.81) (rotation 0.0) (size 2.19 1.587) (radius 1.0)
   (stop_mask auto) (solder_paste off) (clearance 0.0) (function standard)
   (package_pad 0e2a8d54-61a3-4204-9bf1-edf049c03ef1)
   (hole 0e2a8d54-61a3-4204-9bf1-edf049c03ef1 (diameter 1.0)
    (vertex (position 0.0 0.0) (angle 0.0))
   )
  )
  (polygon 2b78c6b2-d906-46c1-b93e-a8f68b43b5c4 (layer top_legend)
   (width 0.25) (fill false) (grab_area true)
   (vertex (position -2.665 5.205) (angle 0.0))
   (vertex (position 2.665 5.205) (angle 0.0))
   (vertex (position 2.665 -5.205) (angle 0.0))
   (vertex (position -2.665 -5.205) (angle 0.0))
   (vertex (position -2.665 5.205) (angle 0.0))
  )
  (polygon b8583314-1b7a-49c5-a258-5618abea441d (layer top_package_outlines)
   (width 0.0) (fill false) (grab_area false)
   (vertex (position -2.54 5.08) (angle 0.0))
   (vertex (position 2.54 5.08) (angle 0.0))
   (vertex (position 2.54 -5.08) (angle 0.0))
   (vertex (position -2.54 -5.08) (angle 0.0))
  )
  (polygon e0b4fa33-f800-442e-b513-7e726b18199c (layer top_courtyard)
   (width 0.0) (fill false) (grab_area false)
   (vertex (position -3.04 5.58) (angle 0.0))
   (vertex (position 3.04 5.58) (angle 0.0))
   (vertex (position 3.04 -5.58) (angle 0.0))
   (vertex (position -3.04 -5.58) (angle 0.0))
  )
  (stroke_text 6a1f12e7-a3b9-47b0-bf31-b8dd211e5af2 (layer top_names)
   (height 1.0) (stroke_width 0.2) (letter_spacing auto) (line_spacing auto)
   (align center bottom) (position 0.0 6.35) (rotation 0.0) (lock false)
   (auto_rotate true) (mirror false) (value "{{NAME}}")
  )
  (stroke_text 7389559e-bc1e-4869-9915-ff063daf8be0 (layer top_values)
   (height 1.0) (stroke_width 0.2) (letter_spacing auto) (line_spacing auto)
   (align center top) (position 0.0 -6.35) (rotation 0.0) (lock false)
   (auto_rotate true) (mirror false) (value "{{VALUE}}")
  )
 )
)
