(librepcb_symbol 07629c99-53f2-4dad-8e95-b95f9781d72e
 (name "Raspberry Pi Pico (SMD)")
 (description "Raspberry Pi Pico SMD module (including test points).")
 (keywords "raspberry,pi,rpi,pico")
 (author "Eric Fossum")
 (version "0.2")
 (created 2022-12-09T18:11:10Z)
 (deprecated false)
 (generated_by "")
 (category e96d0dda-3100-4e68-8c33-e2a5bc80428b)
 (pin 5c65fc67-d10a-4158-910f-d6e9e635884f (name "GPIO0")
  (position 15.24 30.48) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 58084c1c-6b26-4bd9-bd96-b3ed9800ea75 (name "GPIO1")
  (position 15.24 27.94) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 350d8418-15ab-4c87-bdf1-24e0d76d21ad (name "GND")
  (position -15.24 5.08) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 576714d5-7fe6-4544-b000-372e2f064594 (name "GPIO2")
  (position 15.24 25.4) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 22c5f9be-4de2-462b-8ce6-c0fed6050b6a (name "GPIO3")
  (position 15.24 22.86) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 342c0c25-c88f-4fc5-81e7-1554223b820f (name "GPIO4")
  (position 15.24 20.32) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 2b6e501a-d6c2-4a77-b94c-6a21d31a4642 (name "GPIO5")
  (position 15.24 17.78) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin aec954b8-c6de-4ff4-894e-685c31d9ad61 (name "GPIO6")
  (position 15.24 15.24) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin efc6ad78-03cb-44c4-8263-489c7569ffd8 (name "GPIO7")
  (position 15.24 12.7) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin cf3a0de3-fcc7-4914-9a8b-9d2505a00fdc (name "GPIO8")
  (position 15.24 10.16) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 26079f5e-4966-4e87-945d-35e24564d706 (name "GPIO9")
  (position 15.24 7.62) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin dbf70e00-92f1-4fda-b082-c05918ffe93f (name "GPIO10")
  (position 15.24 5.08) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin ff00c9f0-8a5b-4702-afed-b263fbe3219e (name "GPIO11")
  (position 15.24 2.54) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 4bb3bcfe-1bbb-47f1-9122-0cccbca45025 (name "GPIO12")
  (position 15.24 0.0) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 2f7ba14f-fe96-4e63-91bd-6edd640085f4 (name "GPIO13")
  (position 15.24 -2.54) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 2236f866-b95d-43e3-bfaf-cfb21012a87c (name "GPIO14")
  (position 15.24 -5.08) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin ecf1070c-03b3-458c-a7b8-4be85e54d3b9 (name "GPIO15")
  (position 15.24 -7.62) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 54f07ef6-415e-4882-8c55-22a45623f3b1 (name "VBUS_OUT")
  (position -15.24 20.32) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin d5a28e7b-1786-42c9-bb3b-623a03b8cb3e (name "VSYS")
  (position -15.24 10.16) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin cb717dc8-f8b8-4fe2-b9b9-8468c55e964e (name "3V3_EN")
  (position -15.24 30.48) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 41963f23-16de-4c10-8912-61979a49cf61 (name "3V3_OUT")
  (position -15.24 15.24) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 4aab4742-ccc7-4967-85f2-d453a333f891 (name "ADC_VREF")
  (position -15.24 0.0) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin e090368a-1d28-4b57-8063-8bdb4764c0d3 (name "GPIO28")
  (position 15.24 -33.02) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin aaef9fb6-6193-4ec4-ab76-5f153d83d71a (name "GPIO27")
  (position 15.24 -30.48) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin baa67ee1-60cd-457a-9a8e-7fcc563efd78 (name "GPIO26")
  (position 15.24 -27.94) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin ef179285-8c76-45ac-a630-689d17db12fe (name "RUN")
  (position -15.24 25.4) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 5c4ebd5e-cdd3-42eb-8043-0941799e7d7e (name "GPIO22")
  (position 15.24 -25.4) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 080d85fa-e0d4-401c-85c4-fb33ec1d692b (name "GPIO21")
  (position 15.24 -22.86) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 02bec5e0-7207-4ce3-ac0d-d3f55ba86f82 (name "GPIO20")
  (position 15.24 -20.32) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin f6d404bb-e47b-47a0-bd7e-d0c9c1a5a275 (name "GPIO19")
  (position 15.24 -17.78) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 96aaac5a-6699-43f7-b39c-fbe9c872db37 (name "GPIO18")
  (position 15.24 -15.24) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin de64e583-1500-4a60-829d-a1a725abeeff (name "GPIO17")
  (position 15.24 -12.7) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 6e72bb96-071a-4679-963c-177db2f7591a (name "GPIO16")
  (position 15.24 -10.16) (rotation 180.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin d47dd662-1a75-4b6c-bfc5-02a3debb968e (name "SWDIO")
  (position -15.24 -12.7) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin d563c9da-fd01-4aa5-aa48-c14f5f06857a (name "SWCLK")
  (position -15.24 -15.24) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 1fd5fd5a-39fd-4eab-bffa-1b423a06c66c (name "AGND")
  (position -15.24 -5.08) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 011dea42-f69b-4eac-af8b-5d820c46ce5d (name "TP1/USB_GND")
  (position -15.24 -20.32) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin becf56d1-a25f-4147-b966-d06ee08e49a9 (name "TP2/USB_DM")
  (position -15.24 -22.86) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin d91fe8b0-3e83-407d-9b63-f2f4d8128232 (name "TP3/USB_DP")
  (position -15.24 -25.4) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin 1f652cd8-5139-487a-831e-c661b907af65 (name "TP4/SMPS_PS")
  (position -15.24 -27.94) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin fd904def-9399-49a6-9fe5-bd2ff66292cb (name "TP5/LED")
  (position -15.24 -30.48) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (pin ae89eefe-0c35-426a-a11a-00cf8fd5cad3 (name "TP6/BOOTSEL")
  (position -15.24 -33.02) (rotation 0.0) (length 2.54)
  (name_position 3.81 0.0) (name_rotation 0.0) (name_height 2.5)
  (name_align left center)
 )
 (polygon 0030583f-97b0-40c1-8527-2a005a82b122 (layer sym_outlines)
  (width 0.2) (fill false) (grab_area true)
  (vertex (position -12.7 33.02) (angle 0.0))
  (vertex (position 12.7 33.02) (angle 0.0))
  (vertex (position 12.7 -35.56) (angle 0.0))
  (vertex (position -12.7 -35.56) (angle 0.0))
  (vertex (position -12.7 33.02) (angle 0.0))
 )
 (polygon 5cd4a3ab-5427-42bb-a54a-e67b862f6651 (layer sym_outlines)
  (width 0.1) (fill false) (grab_area false)
  (vertex (position -12.7 -17.78) (angle 0.0))
  (vertex (position 1.27 -17.78) (angle 0.0))
  (vertex (position 1.27 -35.56) (angle 0.0))
 )
 (text 7c323984-8ea0-4c4d-83d9-e73236a72abd (layer sym_names) (value "{{NAME}}")
  (align left bottom) (height 2.5) (position -12.7 33.02) (rotation 0.0)
 )
 (text 11d75f3a-d95e-43ff-b916-db0fcf9d7070 (layer sym_values) (value "{{VALUE}}")
  (align left top) (height 2.5) (position -12.7 -35.56) (rotation 0.0)
 )
 (text d2950112-2ab9-4836-992b-d13651e02f39 (layer sym_outlines) (value "Bottom Side Pads")
  (align center top) (height 1.4) (position -5.715 -17.78) (rotation 0.0)
 )
)
