(librepcb_component 01178dc9-fa5a-422e-a75d-9fc168b6b0bf
 (name "RP2040-Tiny")
 (description "Imported from KiCad (RP2040-Tiny:RP2040-Tiny).")
 (keywords "kicad,import")
 (author "KiCad Import")
 (version "0.1")
 (created 2026-03-11T22:38:51Z)
 (deprecated false)
 (generated_by "KiCadImport::RP2040-Tiny::RP2040-Tiny")
 (category e96d0dda-3100-4e68-8c33-e2a5bc80428b)
 (schematic_only false)
 (default_value "{{ MPN or DEVICE }}")
 (prefix "U")
 (signal 0f6d072f-4ac6-4e54-a65a-842c1af9aa0c (name "3V3") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 84cd62d6-0d46-44d9-b731-021645896014 (name "5V") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 90708eaf-55e9-4eb8-9e0d-348d4faeb994 (name "GND") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 876cf1cd-7fe7-4b6b-87ba-493f5e14c0db (name "GPIO0") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal bccb1be1-4247-4cb2-91fe-2567387e192b (name "GPIO14") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal b68be481-a244-45b5-af2b-e4e03c08ddec (name "GPIO15") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 644f2479-0dc3-4ec3-8c50-b1f0fc1c0d11 (name "GPIO26") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 40a58c75-99a4-43ef-83f4-2e6dc2402ab7 (name "GPIO27") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 351cf423-ab63-40e6-a8a9-1e4c18946735 (name "GPIO9") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 2562b70a-d6c8-45d1-a006-ebffa80b5aa9 (name "GPIO10") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal e5a9aebb-05d5-4a16-a06a-1c7176d7b8c4 (name "GPIO11") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 2b72da86-3290-484d-ac2f-b31f45dca5b6 (name "GPIO12") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 48f33a9b-6920-4569-bc1d-a18b190924a1 (name "GPIO13") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal c3b798ab-e342-4545-a28e-3ab90297c2f3 (name "GPIO1") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal b684acef-9fe7-48f5-8a32-d411424b51e0 (name "GPIO28") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 965c0d78-195a-493c-a2ef-02851eec2c6f (name "GPIO29") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 82d281e8-06ad-401a-8e22-a8234310d1f1 (name "GPIO2") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 413af7da-bb15-4e00-a6e2-bf60f57be373 (name "GPIO3") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal ca0182b5-719c-4668-88ac-941ddcedc0f7 (name "GPIO4") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 90c62c49-f5d7-42e0-849e-4ac9581c6ad2 (name "GPIO5") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 7e4f5b18-46e6-4e16-b0a0-360d87dcde20 (name "GPIO6") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal c9acd9fc-9cf2-44e3-8203-7d2fe2967deb (name "GPIO7") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 5c00eb61-ea66-45fb-b489-384d484c700c (name "GPIO8") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (variant 5b29b561-120a-497f-a6f2-d6f7a6ee0008 (norm "")
  (name "default")
  (description "")
  (gate 542c7c96-6f8a-41f2-975d-6bdd27fbfce4
   (symbol a06d51c3-f44d-4215-bda6-bf19a037cd05)
   (position 0.0 0.0) (rotation 0.0) (required true) (suffix "")
   (pin 0313ca0b-c32b-4a69-a321-1ee49b4a38de (signal b684acef-9fe7-48f5-8a32-d411424b51e0) (text signal))
   (pin 0c16bf71-7d84-4835-baae-acef5dff5bb3 (signal 2562b70a-d6c8-45d1-a006-ebffa80b5aa9) (text signal))
   (pin 12bd18e1-1e06-4984-8cee-4e85277e3255 (signal b68be481-a244-45b5-af2b-e4e03c08ddec) (text signal))
   (pin 132ebddc-1fe5-4520-983a-b340bdd4e57e (signal 876cf1cd-7fe7-4b6b-87ba-493f5e14c0db) (text signal))
   (pin 2398d717-be50-495f-af07-5af67552d372 (signal 965c0d78-195a-493c-a2ef-02851eec2c6f) (text signal))
   (pin 3da73bb7-a1de-4c00-9630-d93d3e031f2c (signal 351cf423-ab63-40e6-a8a9-1e4c18946735) (text signal))
   (pin 42e51998-8898-4a26-b754-3b16d8e84140 (signal 7e4f5b18-46e6-4e16-b0a0-360d87dcde20) (text signal))
   (pin 4ea59ddc-71e8-47f3-a696-7034d37c008c (signal 40a58c75-99a4-43ef-83f4-2e6dc2402ab7) (text signal))
   (pin 5d611018-37ca-48f7-a9e0-7e80ef8a7ba2 (signal ca0182b5-719c-4668-88ac-941ddcedc0f7) (text signal))
   (pin 64d2ed81-48c8-49f4-8983-3d1c5738affb (signal c3b798ab-e342-4545-a28e-3ab90297c2f3) (text signal))
   (pin 7333821a-5529-479c-8adc-fdbc06610a05 (signal c9acd9fc-9cf2-44e3-8203-7d2fe2967deb) (text signal))
   (pin 7e412925-ac18-463c-a095-8eb30dea054d (signal 48f33a9b-6920-4569-bc1d-a18b190924a1) (text signal))
   (pin 8995a84e-509c-4d20-a501-33834c557f37 (signal 5c00eb61-ea66-45fb-b489-384d484c700c) (text signal))
   (pin 8d1682a5-0f96-4229-b374-efe658757ca4 (signal 84cd62d6-0d46-44d9-b731-021645896014) (text signal))
   (pin bbf9b445-1612-4b5b-9f52-6030b78efd89 (signal bccb1be1-4247-4cb2-91fe-2567387e192b) (text signal))
   (pin c9dbba18-b4fb-4e69-ac75-4ff24f618c55 (signal 90708eaf-55e9-4eb8-9e0d-348d4faeb994) (text signal))
   (pin e077e563-478e-4fe0-9a89-cee038b1ba45 (signal 90c62c49-f5d7-42e0-849e-4ac9581c6ad2) (text signal))
   (pin e5488ada-5d7d-4579-bbac-f2b14a3079c4 (signal 82d281e8-06ad-401a-8e22-a8234310d1f1) (text signal))
   (pin e7d00a37-52b1-44a8-abd0-a9006c8786f2 (signal 0f6d072f-4ac6-4e54-a65a-842c1af9aa0c) (text signal))
   (pin eafacd69-ce23-438b-8f92-631b56e8262d (signal e5a9aebb-05d5-4a16-a06a-1c7176d7b8c4) (text signal))
   (pin ef378195-2d18-4023-8914-ddbb6c2a6d86 (signal 2b72da86-3290-484d-ac2f-b31f45dca5b6) (text signal))
   (pin f826e109-3c04-4925-8e98-1826b36f4740 (signal 413af7da-bb15-4e00-a6e2-bf60f57be373) (text signal))
   (pin f96b4cdc-6485-4865-81ca-0e5d673ab352 (signal 644f2479-0dc3-4ec3-8c50-b1f0fc1c0d11) (text signal))
  )
 )
)
