(librepcb_component 5e0234ca-8b99-4d09-88be-f57af593bd3b
 (name "OLED-128X64-I2C")
 (description "128x64 Dot Matrix OLED Module based on SSD1306/SSD1309 chip\nVariant with I2C interface")
 (keywords "eagle,import")
 (author "EAGLE Import")
 (version "0.1")
 (created 2025-06-25T16:32:19Z)
 (deprecated false)
 (generated_by "EagleImport::::OLED-128X64-I2C")
 (category a6565eed-ad95-4be7-a29c-39259b1bea5f)
 (schematic_only false)
 (default_value "{{ MPN }}")
 (prefix "DS")
 (signal c62e1141-caf0-4af0-a62e-d25e130cd7ae (name "GND") (role power)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal b269102c-7f65-4a2a-99b7-7ad57195af34 (name "SCL") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal ef8bdd04-b599-4ff1-b26e-d046f8f6db24 (name "SDA") (role inout)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal b2cfb9f0-2fa3-42c4-9daa-0c9019fd8c1c (name "VCC") (role power)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (variant e5b60c56-7790-4366-bd95-f1459aec3ba4 (norm "")
  (name "default")
  (description "")
  (gate 00c0fa4d-bf3e-41e5-a1a0-954a41d34c67
   (symbol c733250c-2339-4401-bc54-0bcf958a69cc)
   (position 0.0 0.0) (rotation 0.0) (required true) (suffix "")
   (pin 10027565-729b-4973-89a4-9a44923c0e7d (signal b269102c-7f65-4a2a-99b7-7ad57195af34) (text signal))
   (pin 5b70507e-68bd-427f-95e4-b392a16c60ab (signal c62e1141-caf0-4af0-a62e-d25e130cd7ae) (text signal))
   (pin 6c1c7f18-2fe0-466f-9de1-1521f79f6de2 (signal b2cfb9f0-2fa3-42c4-9daa-0c9019fd8c1c) (text signal))
   (pin d2f20d5d-6238-471d-9db6-50ecc5e37f87 (signal ef8bdd04-b599-4ff1-b26e-d046f8f6db24) (text signal))
  )
 )
)
