(librepcb_device 5a0990ac-48e7-49fa-a5e2-5ed7c20fc27d
 (name "BC550 (bulk)")
 (description "General-purpose NPN bipolar junction transistor in TO-92 package with 1.27mm pitch, manufactured by several semiconductor companies.")
 (keywords "npn")
 (author "U. Bruhin")
 (version "0.1")
 (created 2023-10-06T10:25:15Z)
 (deprecated false)
 (generated_by "")
 (category e9663545-80dd-4658-9357-d4ef62e55168)
 (component 2e833724-610d-44d8-bd1b-e291e0002736)
 (package 5ee92b46-ab92-4eda-9785-99ef7a36da9f)
 (pad 90f62833-d911-4fe3-b9db-ecef37f0f31b (optional false)
  (signal f560cfa7-f6ac-4d8b-a88f-5a56e33bb563)
 )
 (pad 9114d4a7-61a4-4b64-a50e-148acfe71206 (optional false)
  (signal 83170cf1-eb49-485a-b58e-17f7917d9a16)
 )
 (pad fea307ac-299f-4c4a-a555-eed937427732 (optional false)
  (signal 7881de12-686e-49c0-be89-a40121a77f7d)
 )
 (part "BC550CBU" (manufacturer "onsemi")
  (attribute "V_CEO" (type voltage) (unit volt) (value "45"))
  (attribute "I_C" (type current) (unit milliampere) (value "100"))
  (attribute "POWER_DISSIPATION" (type power) (unit milliwatt) (value "500"))
 )
)
