(librepcb_component a3c283c7-58fd-4b2f-8e9a-a31d218f09ae
 (name "Raspberry Pi Pico (SMD)")
 (description "Raspberry Pi Pico SMD module (including test points).")
 (keywords "raspberry,rpi,pico")
 (author "Eric Fossum")
 (version "0.2")
 (created 2022-12-09T18:25:57Z)
 (deprecated false)
 (generated_by "")
 (category e96d0dda-3100-4e68-8c33-e2a5bc80428b)
 (schematic_only false)
 (default_value "{{DEVICE or COMPONENT}}\n{{MPN}}")
 (prefix "U")
 (signal ac0c8111-4639-4620-9bf6-e284ccb9ec2c (name "GPIO7") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 50407196-6c3d-466f-a9a3-0bfb61be5c11 (name "GPIO16") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal dd37fa68-20eb-4d6d-8db3-d95e84d6d347 (name "GPIO13") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 3c5693c0-1e12-43d0-bd7a-2662a7b362a7 (name "GPIO22") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal b20d74b7-18ba-4e06-927d-7b838b09a748 (name "GPIO10") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal b6e15db4-2b49-46e2-b368-ce98cd134f4e (name "GPIO12") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 57500f61-74e8-4b5f-9264-57cdfc26254b (name "GPIO8") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal e1522abb-2eea-4a75-badb-ebadde128736 (name "GPIO11") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal dc405ee3-ef90-420e-86b7-c310c8163604 (name "GPIO4") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal b03c0578-1c48-4f95-b778-ff5dffa7160a (name "GPIO5") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal c6154311-b201-4dec-a96b-5028338e2a75 (name "GPIO19") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal c5f594ba-dc9b-4f1c-a835-c595e4ed0a51 (name "GPIO1") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 01642d4d-deab-4a1b-8582-cad106587926 (name "GPIO9") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 2485b4bd-2473-47b3-a9d3-121310c1ad86 (name "3V3_EN") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 7dffc2aa-5c56-45c5-96d4-29cefcb4647e (name "3V3_OUT") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal ab32ea3e-7e7b-4a86-ba22-2da4dc19c42a (name "VBUS_OUT") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal ea9d9416-b1fc-4e58-a932-aa390ddbf432 (name "ADC_VREF") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 46460a3d-eba0-4a0c-847b-9734ac8ca404 (name "GPIO17") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 70d12849-9b71-4bc3-a96e-43b37d47d094 (name "GPIO14") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 3a7522fa-c898-405b-a89b-b766fe1c4680 (name "GPIO21") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 48ed9eaf-996f-4b13-90a9-35e52be31b0a (name "GPIO15") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 7dd01c2b-8a8d-4e6d-9f46-a85e1e89eda6 (name "GPIO26") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 52e446a8-82f6-4f1c-bf44-eeec7c94a884 (name "GPIO0") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal c8e60a3e-7aa1-429c-afa6-6054ebc4acb7 (name "GPIO6") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 9530ccf3-2013-4e16-bc44-3554d1cd9470 (name "GPIO18") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 2717b707-2719-4a0d-8910-b1c4ce362b53 (name "VSYS") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal c8274561-3f63-4051-914b-4321c5faad79 (name "GPIO3") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 3306438d-b671-4523-9d70-a10627ee95ab (name "GPIO27") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 9856d75b-e420-4bc9-8c60-fb7b3fb1f7ac (name "RUN") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 251495b8-6982-4c55-8d8f-35d729a21896 (name "GPIO28") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal e40e1278-1893-43a5-8bbd-b519e526afee (name "GPIO2") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal d551fc66-23be-43b3-8412-2544d3226d69 (name "GND") (role passive)
  (required true) (negated false) (clock false) (forced_net "")
 )
 (signal 7d057131-b01a-4164-921b-593ab6123422 (name "GPIO20") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 327cc01e-dea5-4ae1-b4c5-7265ca7427ef (name "SWCLK") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 7d623099-a100-4165-919c-32476e1b8c88 (name "SWDIO") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 29b95257-4051-4678-ad1b-39684b07de0a (name "AGND") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 0cb0d8f8-1b6b-4cba-92b9-c45432a8ab40 (name "TP1/USB_GND") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal b4b79e73-7297-4a7e-adf0-db36d85ee352 (name "TP2/USB_DM") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal c3510daf-f4e2-4dab-8d51-50e40f37f563 (name "TP3/USB_DP") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 49011584-1608-4236-b4b1-8fbaef0bc21e (name "TP4/SMPS_PS") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal d2e33773-7518-421c-9493-9f4a66b89156 (name "TP5/LED") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (signal 17410acb-ddd8-420a-b88d-b6e59a180aef (name "TP6/BOOTSEL") (role passive)
  (required false) (negated false) (clock false) (forced_net "")
 )
 (variant c61f7168-bb43-4cfb-8cef-b9a4628fa3e1 (norm "")
  (name "default")
  (description "")
  (gate b133fcc3-903c-4238-b3b8-a34f510e5ae9
   (symbol 07629c99-53f2-4dad-8e95-b95f9781d72e)
   (position 0.0 0.0) (rotation 0.0) (required true) (suffix "")
   (pin 011dea42-f69b-4eac-af8b-5d820c46ce5d (signal 0cb0d8f8-1b6b-4cba-92b9-c45432a8ab40) (text signal))
   (pin 02bec5e0-7207-4ce3-ac0d-d3f55ba86f82 (signal 7d057131-b01a-4164-921b-593ab6123422) (text signal))
   (pin 080d85fa-e0d4-401c-85c4-fb33ec1d692b (signal 3a7522fa-c898-405b-a89b-b766fe1c4680) (text signal))
   (pin 1f652cd8-5139-487a-831e-c661b907af65 (signal 49011584-1608-4236-b4b1-8fbaef0bc21e) (text signal))
   (pin 1fd5fd5a-39fd-4eab-bffa-1b423a06c66c (signal 29b95257-4051-4678-ad1b-39684b07de0a) (text signal))
   (pin 2236f866-b95d-43e3-bfaf-cfb21012a87c (signal 70d12849-9b71-4bc3-a96e-43b37d47d094) (text signal))
   (pin 22c5f9be-4de2-462b-8ce6-c0fed6050b6a (signal c8274561-3f63-4051-914b-4321c5faad79) (text signal))
   (pin 26079f5e-4966-4e87-945d-35e24564d706 (signal 01642d4d-deab-4a1b-8582-cad106587926) (text signal))
   (pin 2b6e501a-d6c2-4a77-b94c-6a21d31a4642 (signal b03c0578-1c48-4f95-b778-ff5dffa7160a) (text signal))
   (pin 2f7ba14f-fe96-4e63-91bd-6edd640085f4 (signal dd37fa68-20eb-4d6d-8db3-d95e84d6d347) (text signal))
   (pin 342c0c25-c88f-4fc5-81e7-1554223b820f (signal dc405ee3-ef90-420e-86b7-c310c8163604) (text signal))
   (pin 350d8418-15ab-4c87-bdf1-24e0d76d21ad (signal d551fc66-23be-43b3-8412-2544d3226d69) (text signal))
   (pin 41963f23-16de-4c10-8912-61979a49cf61 (signal 7dffc2aa-5c56-45c5-96d4-29cefcb4647e) (text signal))
   (pin 4aab4742-ccc7-4967-85f2-d453a333f891 (signal ea9d9416-b1fc-4e58-a932-aa390ddbf432) (text signal))
   (pin 4bb3bcfe-1bbb-47f1-9122-0cccbca45025 (signal b6e15db4-2b49-46e2-b368-ce98cd134f4e) (text signal))
   (pin 54f07ef6-415e-4882-8c55-22a45623f3b1 (signal ab32ea3e-7e7b-4a86-ba22-2da4dc19c42a) (text signal))
   (pin 576714d5-7fe6-4544-b000-372e2f064594 (signal e40e1278-1893-43a5-8bbd-b519e526afee) (text signal))
   (pin 58084c1c-6b26-4bd9-bd96-b3ed9800ea75 (signal c5f594ba-dc9b-4f1c-a835-c595e4ed0a51) (text signal))
   (pin 5c4ebd5e-cdd3-42eb-8043-0941799e7d7e (signal 3c5693c0-1e12-43d0-bd7a-2662a7b362a7) (text signal))
   (pin 5c65fc67-d10a-4158-910f-d6e9e635884f (signal 52e446a8-82f6-4f1c-bf44-eeec7c94a884) (text signal))
   (pin 6e72bb96-071a-4679-963c-177db2f7591a (signal 50407196-6c3d-466f-a9a3-0bfb61be5c11) (text signal))
   (pin 96aaac5a-6699-43f7-b39c-fbe9c872db37 (signal 9530ccf3-2013-4e16-bc44-3554d1cd9470) (text signal))
   (pin aaef9fb6-6193-4ec4-ab76-5f153d83d71a (signal 3306438d-b671-4523-9d70-a10627ee95ab) (text signal))
   (pin ae89eefe-0c35-426a-a11a-00cf8fd5cad3 (signal 17410acb-ddd8-420a-b88d-b6e59a180aef) (text signal))
   (pin aec954b8-c6de-4ff4-894e-685c31d9ad61 (signal c8e60a3e-7aa1-429c-afa6-6054ebc4acb7) (text signal))
   (pin baa67ee1-60cd-457a-9a8e-7fcc563efd78 (signal 7dd01c2b-8a8d-4e6d-9f46-a85e1e89eda6) (text signal))
   (pin becf56d1-a25f-4147-b966-d06ee08e49a9 (signal b4b79e73-7297-4a7e-adf0-db36d85ee352) (text signal))
   (pin cb717dc8-f8b8-4fe2-b9b9-8468c55e964e (signal 2485b4bd-2473-47b3-a9d3-121310c1ad86) (text signal))
   (pin cf3a0de3-fcc7-4914-9a8b-9d2505a00fdc (signal 57500f61-74e8-4b5f-9264-57cdfc26254b) (text signal))
   (pin d47dd662-1a75-4b6c-bfc5-02a3debb968e (signal 7d623099-a100-4165-919c-32476e1b8c88) (text signal))
   (pin d563c9da-fd01-4aa5-aa48-c14f5f06857a (signal 327cc01e-dea5-4ae1-b4c5-7265ca7427ef) (text signal))
   (pin d5a28e7b-1786-42c9-bb3b-623a03b8cb3e (signal 2717b707-2719-4a0d-8910-b1c4ce362b53) (text signal))
   (pin d91fe8b0-3e83-407d-9b63-f2f4d8128232 (signal c3510daf-f4e2-4dab-8d51-50e40f37f563) (text signal))
   (pin dbf70e00-92f1-4fda-b082-c05918ffe93f (signal b20d74b7-18ba-4e06-927d-7b838b09a748) (text signal))
   (pin de64e583-1500-4a60-829d-a1a725abeeff (signal 46460a3d-eba0-4a0c-847b-9734ac8ca404) (text signal))
   (pin e090368a-1d28-4b57-8063-8bdb4764c0d3 (signal 251495b8-6982-4c55-8d8f-35d729a21896) (text signal))
   (pin ecf1070c-03b3-458c-a7b8-4be85e54d3b9 (signal 48ed9eaf-996f-4b13-90a9-35e52be31b0a) (text signal))
   (pin ef179285-8c76-45ac-a630-689d17db12fe (signal 9856d75b-e420-4bc9-8c60-fb7b3fb1f7ac) (text signal))
   (pin efc6ad78-03cb-44c4-8263-489c7569ffd8 (signal ac0c8111-4639-4620-9bf6-e284ccb9ec2c) (text signal))
   (pin f6d404bb-e47b-47a0-bd7e-d0c9c1a5a275 (signal c6154311-b201-4dec-a96b-5028338e2a75) (text signal))
   (pin fd904def-9399-49a6-9fe5-bd2ff66292cb (signal d2e33773-7518-421c-9493-9f4a66b89156) (text signal))
   (pin ff00c9f0-8a5b-4702-afed-b263fbe3219e (signal e1522abb-2eea-4a75-badb-ebadde128736) (text signal))
  )
 )
)
